City of Conway, Arkansas

Mayor’s Office

1111 Main Street

Conway, AR 72032

501.450.6100

Office of the Mayor

City of Conway

Bid Tabulation Sheet

[www.conwayarkansas.gov](http://www.conwayarkansas.gov)



Number of Bids Received - 2

Opened by: Jamie Brice and Jacob Reynolds

|  |
| --- |
| Bid Number: 2022-03 – Annual Bid Concrete Work New ConstructionBid Opening Date: Tuesday, December 14, 2021 @ 10:00am  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Bidder’s Name  | 4” x 2’ Wide Roll Curb & Gutter -per lineal foot | 6” High x 1.5 Wide Upright Curb & Gutter – Per lineal foot | 6” High x 2’ High Upright Curb & Gutter – Per lineal foot  | Inlet Top – Each | Inlet Throat-Each | Inlet Barrel - Each | Concrete Curb Inlet 4’ Extension | Sidewalk/DrivewayVariable widths (est. 3000 sq. yd.)Per sq. yd. | Concrete Pavement Avg 8” Variable widths (est 3000 SY) | Concrete Pavement, Undercut of Unsuitable Material Per cu. Yd. |
| Evatt Construction | **5.50** | **5.00** | **5.50** | **900** | **300** | **900** | **400** | **22.50** | **22.50** | **55** |
| JCI | 5.50 | 5.50 | 5.50 | 800 | 200 | 800 | 400 | 20 | 20 | 40 |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |

For additional information regarding this bid; please contact Kurt Jones @ kurt.jones@conwayarkansas.gov 501.450.6165.

|  |
| --- |
| Bid Number: 2022-03 – Annual Bid Concrete Work Remove/ReplaceBid Opening Date: Tuesday, December 14, 2021 @ 10:00am  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Bidder’s Name  | 4” x 2’ Wide Roll Curb & Gutter -per lineal foot | 6” High x 1.5 Wide Upright Curb & Gutter – Per lineal foot | 6” High x 2’ High Upright Curb & Gutter – Per lineal foot  | Inlet Top – Each | Inlet Throat-Each | Inlet Barrel - Each | Concrete Curb Inlet 4’ Extension | Sidewalk/DrivewayVariable widths (est. 3000 sq. yd.)Per sq. yd. | Concrete Pavement Avg 8” Variable widths (est 3000 SY) | Concrete Pavement, Undercut of Unsuitable Material Per cu. Yd. |
| Evatt Construction | 22 | 22 | 22 | 1800 | 600 | 1800 | 800 | 60 | 120 | 225 |
| JCI | 15.50 | 15.50 | 15.50 | 1500 | 500 | 1500 | 500 | 50 | 75 | 45 |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |